How to Connect a Card Reader via Wi-Fi and Configure the Network (readers received before 2025)

This article walks through connecting a card reader to Wi-Fi or Ethernet, locating its IP address, and editing the host file so it can communicate properly.

Connecting through Wi-Fi
Power on the device. Make sure device is plugged in and turned onOpen the admin menu. For Desk 3500/2600 and Move 5000 press the ¤ key (silver target button above the number 3). For Lane 3000/5000/7000 Press the F keySelect "Admin Mode" on the screenEnter the password. You will be prompted for a password (123456A)Confirm. Press the green circle once password is enteredNavigate to Wi-Fi scan. Navigate to Control Panel > Terminal Settings > Comm means > Wi-Fi > Scan networksSelect your network. Select the network that you intend to connect to and enter the password
Connecting through Ethernet


Connect Card reader to internet router.


Locating IP Address — Wi-Fi
Open Wi-Fi status display. Navigate to Control Panel > Terminal Settings > Comm means > Wi-Fi > Status > DisplayScroll down to "IP: " fieldNotate IP as it will need to be placed into host file
Locating IP Address — Ethernet
Open Ethernet settings. Navigate to Control Panel > Terminal Settings > Comm means > EthernetScroll down to "IP: " fieldNotate IP as it will need to be placed into host file
Editing Host File
Locate notepad application. Notepad, notepad ++, etc. Right click application and select "Run as administrator"Go to File > OpenNavigate to host file at: Local Disk (C:)/Windows/System32/drivers/etc/ will appear blank (change txt.files to all files) /hostsPaste correct mapping in host file. Paste " [Insert IP Address Here] . Hit the Tab Key on your keyboard. Then enter in "secure.wsstxn.com" in host file (without quotes or brackets)Save file

Expected Result


The card reader is connected to Wi-Fi (or Ethernet) and its IP address is mapped to secure.wsstxn.com in the host file.


💡 TipWhen navigating to the host file, it will appear blank — change txt.files to all files to view it.





