Overview
Barcoding serialized inventory allows for quick
and easy review
of firearm information via scanning.
 
The Barcode
Generator is a tool used
to create scalable barcodes to track
your on-hand inventory. It permits you to enter
a serial number
or Handling Unit
Name and print
a barcode label and
apply it to an inventory tag or box.
The tool requires that you own a barcode
label printer (for small
labels) or use printable labels
on a larger printer.
 
Software Needed
•     
 Barcode Generator
 
Hardware Needed
•     
Barcode Printer
o  
Single Barcode Printer
o  
1D, 2D, or QR (1D minimum)
o  
Suggested Printers
▪      DYMO LabelWriter 450 Turbo
Thermal Label Printer










                                    ▪     
Seiko Instruments Smart
Label Printer 620,
USB, PC/Mac


 


                              
•     
Scanner
o  
1D, 2D or QR scanner
(1D minimum)
o  
Bluetooth or Wireless
o  
Suggested Scanners
▪    Rhorawill Handheld Red Light CCD Barcode Scanner|500 Times/Sec USB 1D Bar Code
Reader






 


▪     
Esky ES017 Handheld USB Wired Barcode
Scanner - Automatic 1D and 2D QR Code  Reader




                                          



Supplies Needed

                                  •     Dymo Labels 30320 (1 1/8" X 3 1/2")
                                          

                                  

                                   •      Avery Address Labels 4150 (1 1 8” x 3 1 2”)

                                          



      
Instructions for How to Create a Barcode
1.       
From the software portal main menu, click
Barcode Generator.






     2.      
The Barcode Generator screen
will now display. To generate a barcode, enter
the serial number or Handling Unit
Name in the
Enter Serial Number
or ID field.









      3.       The information as entered will
create a barcode
for display. To print, select
the Print button.








Coming Soon
•     
Multi-Serial Number to Multi-Barcode generator






